,WIND RESISTANCE##OTHER##,WIDTH_LVM##LENGTH##MILLIMETERS,WEIGHT##MASS##KILOGRAMS,URL##OTHER##,THERMAL TRASMITTANCE##HVAC_COEFFICIENT_OF_HEAT_TRANSFER##WATTS_PER_SQUARE_METER_KELVIN,TECHNICAL SHEET##OTHER##,PRODUCT SHEET##OTHER##,PANIC HANDLE##OTHER##,NOISE REDUCTION##OTHER##,Model##OTHER##,Manufacturer##OTHER##,MATERIAL DESCRIPTION##OTHER##,MANUAL HANDLE##OTHER##,HEIGHT_HVM##LENGTH##MILLIMETERS,H Panel##LENGTH##MILLIMETERS,H Handle##LENGTH##MILLIMETERS,H Frame##LENGTH##MILLIMETERS,Function##OTHER##,Height##LENGTH##MILLIMETERS,Wall Closure##OTHER##,Width##LENGTH##MILLIMETERS,FIRE RESISTANCE UNI EN 1634-1##OTHER##,FINISHING##OTHER##,Description##OTHER##,BIM USER MANUAL##OTHER##,BIM BADGE##OTHER##,BIM AUTHOR##OTHER##,Analytic Construction##OTHER##,AIR PERMEABILITY##OTHER##
LVM 1000 - HVM 2150,C4,1000.000000000000,35.000000000000,https://www.dierre.com/en,1.800000000000,https://www.dierre.com/en/prodotti/porte-tagliafuoco/new-idra-1b,https://bim.archiproducts.com/en/products/dierre/fire-door-new-idra_382867,1,19 dB,NEW IDRA 1B,Dierre,"Steel fire door, which guarantees maximum safety of the rooms and a pleasant presence, due to the particular coplanarity of the door with the frame.",0,2150.000000000000,2143.000000000000,1000.000000000000,2148.000000000000,0,2150.000000000000,0,1000.000000000000,EI 60,DIERRE_AVORIO,One leaf flexible and safe fire door,https://bimcad.edilportale.com/DIERRE-DOOR-BIM-USER-MANUAL-DIERRE-bim.pdf,https://bim.archiproducts.com/en/badge/bim-archiproducts-featured_658700/about,https://bim.archiproducts.com,<None>,Classe 4
