,WIDTH_LVM##LENGTH##MILLIMETERS,WEIGHT##MASS##KILOGRAMS,VISIBILITY DOOR##OTHER##,URL##OTHER##,Thickness##LENGTH##MILLIMETERS,TECHNICAL SHEET##OTHER##,PRODUCT SHEET##OTHER##,PANIC HANDLE FINISH##OTHER##,PANIC HANDLE##OTHER##,ONLY PANEL##OTHER##,Manufacturer##OTHER##,Model##OTHER##,Rough Width##LENGTH##MILLIMETERS,MATERIAL DESCRIPTION##OTHER##,L_Guida##LENGTH##MILLIMETERS,H_Door##LENGTH##MILLIMETERS,HEIGHT_HVM##LENGTH##MILLIMETERS,Function##OTHER##,Partenza B##OTHER##,Partenza A##OTHER##,FIRE RESISTANCE UNI EN 1634-1##OTHER##,FINISHING##OTHER##,Description##OTHER##,BIM USER MANUAL##OTHER##,BIM BADGE##OTHER##,BIM AUTHOR##OTHER##,Asse porta##LENGTH##MILLIMETERS,Assembly Code##OTHER##,Analytic Construction##OTHER##,Rough Height##LENGTH##MILLIMETERS,Height##LENGTH##MILLIMETERS,Wall Closure##OTHER##,Width##LENGTH##MILLIMETERS
ONLY SLIDING DOOR,5000.000000000000,50.000000000000,0,https://www.dierre.com/en,80.000000000000,https://www.dierre.com/en/prodotti/porte-tagliafuoco/rolling-1b,https://www.archiproducts.com/en/products/dierre/fire-door-rolling_382868,RED,1,1,Dierre,ROLLING,5350.000000000000,"Blind door 85 mm thick, built from one or more modular panels made of pre-painted galvanized steel with 7/10 thick double sheet structure and protective film. Internal filling of the door with high density rock wool mattress",10650.000000000000,2200.000000000000,3300.000000000000,0,1,0,EI 120,DIERRE_AVORIO,Horizontal sliding door fireproof steel,,https://bim.archiproducts.com/en/badge/bim-archiproducts-featured_658700/about,https://bim.archiproducts.com,14.000000000000,,<None>,3575.000000000001,3300.000000000000,0,5000.000000000000
WITH DOOR,5000.000000000000,50.000000000000,1,https://www.dierre.com/en,80.000000000000,https://www.dierre.com/en/prodotti/porte-tagliafuoco/rolling-1b,https://www.archiproducts.com/en/products/dierre/fire-door-rolling_382868,RED,1,0,Dierre,ROLLING,5350.000000000000,"Blind door 85 mm thick, built from one or more modular panels made of pre-painted galvanized steel with 7/10 thick double sheet structure and protective film. Internal filling of the door with high density rock wool mattress",10650.000000000000,2200.000000000000,3300.000000000000,0,1,0,EI 120,DIERRE_AVORIO,Horizontal sliding door fireproof steel,https://img.edilportale.com/bim/DIERRE-DOOR-BIM-USER-MANUAL-DIERRE-bim.pdf,https://bim.archiproducts.com/en/badge/bim-archiproducts-featured_658700/about,https://bim.archiproducts.com,14.000000000000,,<None>,3575.000000000001,3300.000000000000,0,5000.000000000000
