,Width reinforcement##LENGTH##MILLIMETERS,Width passage##LENGTH##MILLIMETERS,Width Panel##LENGTH##MILLIMETERS,Trasmittanza luminosa##OTHER##,URL##OTHER##,L##LENGTH##MILLIMETERS,Internal panel visible y/n##OTHER##,Height Panel##LENGTH##MILLIMETERS,H##LENGTH##MILLIMETERS,Commenti sul tipo##OTHER##,Spessore##LENGTH##MILLIMETERS,Resistenza termica (R)##HVAC_THERMAL_RESISTANCE##SQUARE_METER_KELVINS_PER_WATT,TECHNICAL SHEET##OTHER##,Indice di riscaldamento alla radiazione solare##OTHER##,Sliding Door Symbol_Visibility##OTHER##,Larghezza approssimativa##LENGTH##MILLIMETERS,Altezza approssimativa##LENGTH##MILLIMETERS,PRODUCT SHEET##OTHER##,PANEL MATERIAL##OTHER##,Modello##OTHER##,Produttore##OTHER##,MATERIAL DESCRIPTION##OTHER##,Nota chiave##OTHER##,Altezza##LENGTH##MILLIMETERS,Chiusura muro##OTHER##,Larghezza##LENGTH##MILLIMETERS,Coefficiente di scambio termico (U)##HVAC_COEFFICIENT_OF_HEAT_TRANSFER##WATTS_PER_SQUARE_METER_KELVIN,Handle Height##LENGTH##MILLIMETERS,HANDLE COMMENTS##OTHER##,Funzione##OTHER##,FRAME MATERIAL##OTHER##,Definisci proprietà termiche per##OTHER##,Descrizione##OTHER##,DOOR HANDLE MATERIAL##OTHER##,BIM USER MANUAL##OTHER##,BIM BADGE##OTHER##,BIM AUTHOR##OTHER##,Codice assieme##OTHER##,Costruzione analitica##OTHER##,AVAILABLE FINISHES##OTHER##,AVAILABLE DIMENSIONS##OTHER##
LNL 800 - LNH 2100,768.000000000000,740.000000000001,770.000000000000,0,https://www.dierre.com,800.000000000000,1,2285.000000000000,2300.000000000000,,74.000000000000,0.455702653451,https://www.dierre.com/en/product/safety-doors/teknica/under/,0,1,1725.000000000000,2357.000000000000,https://www.archiproducts.com/en/products/dierre/galvanized-steel-safety-door-with-concealed-hinges-under_723088,Aluminum - Dierre,Under0,DIERRE,Melamine-faced chipboard,,2300.000000000000,0,800.000000000000,2.194648649500,1050.000000000000,"Different handle types available; please, for further info, refer to the TECHNICAL SHEET or contact DIERRE technical departement",0,Aluminum - Dierre,1,"Teknica Under by Dierre is a top-performing safety door with an ultra-slim threshold for easy passage, advanced thermal and acoustic insulation, and a sleek design. It offers superior security without sacrificing style, making it the ideal solution for contemporary homes.",Aluminum - Dierre,https://bimcad.edilportale.com/DIERRE-BIM-USER-MANUAL-DIERRE-bim.pdf,https://bim.archiproducts.com/en/badge/bim-archiproducts-featured_658700/about,https://bim.archiproducts.com/,,<None>,"Different finishes and colours available; please, for further info, refer to the TECHNICAL SHEET or contact DIERRE technical departement",Width: 500-1050 mm | Height: 1600-2500 mm
