,WIDTH_LP##LENGTH##MILLIMETERS,WEIGHT##MASS##KILOGRAMS,Visual Light Transmittance##OTHER##,URL##OTHER##,THERMAL TRASMITTANCE##HVAC_COEFFICIENT_OF_HEAT_TRANSFER##WATTS_PER_SQUARE_METER_KELVIN,TECHNICAL SHEET##OTHER##,PRODUCT SHEET##OTHER##,MATERIAL DESCRIPTION##OTHER##,Handle##OTHER##,H_Handle##LENGTH##MILLIMETERS,HEIGHT_HP##LENGTH##MILLIMETERS,FIRE RESISTANCE UNI EN 1634-1##OTHER##,FINISHING##OTHER##,FILOMURO##OTHER##,ELECTRIC HANDLE##OTHER##,DOOR COVER_PANNEL##OTHER##,Cover##LENGTH##MILLIMETERS,Type Comments##OTHER##,Thickness##LENGTH##MILLIMETERS,Thermal Resistance (R)##HVAC_THERMAL_RESISTANCE##SQUARE_METER_KELVIN_PER_WATT,Solar Heat Gain Coefficient##OTHER##,Rough Width##LENGTH##MILLIMETERS,Rough Height##LENGTH##MILLIMETERS,Model##OTHER##,Manufacturer##OTHER##,Keynote##OTHER##,Height##LENGTH##MILLIMETERS,Wall Closure##OTHER##,Width##LENGTH##MILLIMETERS,Heat Transfer Coefficient (U)##HVAC_COEFFICIENT_OF_HEAT_TRANSFER##WATTS_PER_SQUARE_METER_KELVIN,Handle Height##LENGTH##MILLIMETERS,Function##OTHER##,Description##OTHER##,BIM USER MANUAL##OTHER##,BIM BADGE##OTHER##,BIM AUTHOR##OTHER##,Assembly Code##OTHER##,Analytic Construction##OTHER##,A##LENGTH##MILLIMETERS
LNL 900 - LNH 2100,1200.000000000000,55.000000000000,0,https://www.dierre.com,4.300000000000,https://www.dierre.com/en/prodotti/porte-tagliafuoco/visual-1b,https://www.archiproducts.com/it/prodotti/dierre/porta-tagliafuoco-visual_382869,"Glazed door 80 mm thick, built with perimeter structure in painted galvanized steel, with thermal break profile with calcium silicate insulation.",0,1000.000000000000,2100.000000000000,REI 120,DIERRE_AVORIO,1,1,0,0.000000000000,,63.000000000000,0.000000000000,0,1358.000000000000,2179.000000000000,VISUAL,Dierre,,2100.000000000000,0,1200.000000000000,1.300000000000,1000.000000000000,1,One-leaf steel fire-resistant glass door,https://img.edilportale.com/bim/DIERRE-DOOR-BIM-USER-MANUAL-DIERRE-bim.pdf,https://bim.archiproducts.com/en/badge/bim-archiproducts-featured_658700/about,https://bim.archiproducts.com/,,<None>,63.000000000000
